(footprint "Pin0.9mm" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "solder Pin_ with flat fork, hole diameter 0.9mm, length 10.0mm, width 2.4mm")
  (tags "solder Pin_ with flat fork")
  (property "Sheetfile" "tangentbord1.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Generic connector, single row, 01x01, script generated")
  (property "ki_keywords" "connector")
  (attr through_hole)
  (fp_text reference "E6" (at 0 1.95) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 64ac2c78-2081-4dfe-abd8-c7969671eb2e)
  )
  (fp_text value "Conn_01x01_Pin" (at 0 -2.05) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a1037d8d-e47a-485a-9c48-4dc726a40f93)
  )
  (fp_text user "${REFERENCE}" (at 3.25 0.3) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 7d675050-eaca-443a-8874-86ee75c238fa)
  )
  (fp_line (start -1.2 -0.25) (end -1.2 0.25)
    (stroke (width 0.12) (type solid)) (layer "F.Fab") (tstamp f2ae5a7d-1156-4326-b24b-00bc9dba310f))
  (fp_line (start -1.2 0.25) (end 1.2 0.25)
    (stroke (width 0.12) (type solid)) (layer "F.Fab") (tstamp 19faf3db-a040-43e2-840b-24b06637bd7a))
  (fp_line (start 1.2 -0.25) (end -1.2 -0.25)
    (stroke (width 0.12) (type solid)) (layer "F.Fab") (tstamp 1738a114-d7ca-4299-ad0e-47c1060309aa))
  (fp_line (start 1.2 0.25) (end 1.2 -0.25)
    (stroke (width 0.12) (type solid)) (layer "F.Fab") (tstamp 97f78280-45e5-45f0-98ab-89907f21a22a))
  (pad "1" thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask") (tstamp c037ae89-3f7d-43df-9c1d-936025184702))
  (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.9mm_L10.0mm_W2.4mm_FlatFork.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
