(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "ITSYBITSY_RP2040" (in_bom yes) (on_board yes)
    (property "Reference" "U1" (at 3.81 41.91 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "ITSYBITSY RP2040" (at 0 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Footprints:ITSYBITSY BREAKOUT" (at 24.13 -20.32 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 5.08 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ITSYBITSY_RP2040_1_1"
      (rectangle (start -17.78 39.37) (end 17.78 -16.51)
        (stroke (width 0) (type default))
        (fill (type background))
      )
      (pin input line (at -17.78 35.56 0) (length 2.54)
        (name "RESET" (effects (font (size 1.27 1.27))))
        (number "0" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -17.78 31.75 0) (length 2.54)
        (name "3.3V" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 -2.54 0) (length 2.54)
        (name "SCK" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 -6.35 0) (length 2.54)
        (name "MOSI" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 -10.16 0) (length 2.54)
        (name "MISO" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 -13.97 0) (length 2.54)
        (name "D2" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -3.81 -16.51 90) (length 2.54)
        (name "SWDIO" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 0 -16.51 90) (length 2.54)
        (name "SWCLK" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 3.81 -16.51 90) (length 2.54)
        (name "D3" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -13.97 180) (length 2.54)
        (name "RX" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -10.16 180) (length 2.54)
        (name "TX" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -6.35 180) (length 2.54)
        (name "SDA" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -17.78 27.94 0) (length 2.54)
        (name "3.3V" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -2.54 180) (length 2.54)
        (name "SCL" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 1.27 180) (length 2.54)
        (name "D5" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 5.08 180) (length 2.54)
        (name "D7" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 8.89 180) (length 2.54)
        (name "D9" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 12.7 180) (length 2.54)
        (name "D10" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 16.51 180) (length 2.54)
        (name "D11" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 20.32 180) (length 2.54)
        (name "D12" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 24.13 180) (length 2.54)
        (name "D13" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.78 27.94 180) (length 2.54)
        (name "VBUS" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.78 31.75 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -17.78 24.13 0) (length 2.54)
        (name "VHI" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.78 35.56 180) (length 2.54)
        (name "VBAT" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 20.32 0) (length 2.54)
        (name "A0" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 16.51 0) (length 2.54)
        (name "A1" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 12.7 0) (length 2.54)
        (name "A2" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 8.89 0) (length 2.54)
        (name "A3" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 5.08 0) (length 2.54)
        (name "D24" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 1.27 0) (length 2.54)
        (name "D25" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MX_SW_SOCKET_RGB" (in_bom yes) (on_board yes)
    (property "Reference" "S4" (at 11.43 -1.27 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MX_SW_SOCKET_LED" (at 21.59 10.16 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Footprint" "Footprints:MX_SW_SOCKET_LED" (at 26.67 7.62 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 3.81 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MX_SW_SOCKET_RGB_0_1"
      (polyline
        (pts
          (xy -1.27 5.08)
          (xy -0.8247 5.0799)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 5.08)
          (xy 0.8247 5.0801)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -10.16 6.35)
          (xy -10.16 8.89)
          (xy -7.62 8.89)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -7.62 -10.16)
          (xy -10.16 -10.16)
          (xy -10.16 -7.62)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 7.62 8.89)
          (xy 10.16 8.89)
          (xy 10.16 6.35)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 10.16 -7.62)
          (xy 10.16 -10.16)
          (xy 7.62 -10.16)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
    )
    (symbol "MX_SW_SOCKET_RGB_1_1"
      (rectangle (start -6.35 0) (end 6.35 -8.89)
        (stroke (width 0) (type default))
        (fill (type background))
      )
      (rectangle (start -3.81 7.62) (end 3.81 1.27)
        (stroke (width 0) (type default))
        (fill (type background))
      )
      (circle (center -0.6173 5.0896) (radius 0.1705)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -1.27 5.08)
          (xy -1.27 7.62)
        )
        (stroke (width 0) (type dot))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.5184 5.2126)
          (xy 0.4381 5.7713)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 7.62)
          (xy 1.27 5.08)
        )
        (stroke (width 0) (type dot))
        (fill (type none))
      )
      (circle (center 0.6471 5.08) (radius 0.1705)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (text "NEOPIXEL" (at 0 -1.27 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "SWITCH" (at 0 2.54 0)
        (effects (font (size 1.27 1.27)))
      )
      (pin bidirectional line (at -1.27 10.16 270) (length 2.54)
        (name "L" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 1.27 10.16 270) (length 2.54)
        (name "R" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -11.43 90) (length 2.54)
        (name "G" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 -11.43 90) (length 2.54)
        (name "5V" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 8.89 -3.81 180) (length 2.54)
        (name "DIN" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -8.89 -3.81 0) (length 2.54)
        (name "DOUT" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MX_SW_SOCKET_RGB_1" (in_bom yes) (on_board yes)
    (property "Reference" "S5" (at 11.43 -1.27 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "MX_SW_SOCKET_LED" (at 20.32 7.62 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Footprint" "Footprints:MX_SW_SOCKET_LED" (at 25.4 5.08 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 3.81 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MX_SW_SOCKET_RGB_1_0_1"
      (polyline
        (pts
          (xy -1.27 5.08)
          (xy -0.8247 5.0799)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 5.08)
          (xy 0.8247 5.0801)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -10.16 6.35)
          (xy -10.16 8.89)
          (xy -7.62 8.89)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -7.62 -10.16)
          (xy -10.16 -10.16)
          (xy -10.16 -7.62)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 7.62 8.89)
          (xy 10.16 8.89)
          (xy 10.16 6.35)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 10.16 -7.62)
          (xy 10.16 -10.16)
          (xy 7.62 -10.16)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
    )
    (symbol "MX_SW_SOCKET_RGB_1_1_1"
      (rectangle (start -6.35 0) (end 6.35 -8.89)
        (stroke (width 0) (type default))
        (fill (type background))
      )
      (rectangle (start -3.81 7.62) (end 3.81 1.27)
        (stroke (width 0) (type default))
        (fill (type background))
      )
      (circle (center -0.6173 5.0896) (radius 0.1705)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -1.27 5.08)
          (xy -1.27 7.62)
        )
        (stroke (width 0) (type dot))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.5184 5.2126)
          (xy 0.4381 5.7713)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 7.62)
          (xy 1.27 5.08)
        )
        (stroke (width 0) (type dot))
        (fill (type none))
      )
      (circle (center 0.6471 5.08) (radius 0.1705)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (text "NEOPIXEL" (at 0 -1.27 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "SWITCH" (at 0 2.54 0)
        (effects (font (size 1.27 1.27)))
      )
      (pin bidirectional line (at -1.27 10.16 270) (length 2.54)
        (name "L" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 1.27 10.16 270) (length 2.54)
        (name "R" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -11.43 90) (length 2.54)
        (name "G" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 -11.43 90) (length 2.54)
        (name "5V" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 8.89 -3.81 180) (length 2.54)
        (name "DIN" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -8.89 -3.81 0) (length 2.54)
        (name "DOUT" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MX_SW_SOCKET_RGB_REV" (in_bom yes) (on_board yes)
    (property "Reference" "S6" (at 12.7 -3.2259 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MX_SW_SOCKET_RGB_REV" (at 22.86 8.89 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Footprint" "Footprints:MX_SW_SOCKET_LED_REV" (at 27.94 6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 3.81 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MX_SW_SOCKET_RGB_REV_0_1"
      (polyline
        (pts
          (xy -1.27 5.08)
          (xy -0.8247 5.0799)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 5.08)
          (xy 0.8247 5.0801)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -10.16 6.35)
          (xy -10.16 8.89)
          (xy -7.62 8.89)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -7.62 -10.16)
          (xy -10.16 -10.16)
          (xy -10.16 -7.62)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 7.62 8.89)
          (xy 10.16 8.89)
          (xy 10.16 6.35)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 10.16 -7.62)
          (xy 10.16 -10.16)
          (xy 7.62 -10.16)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
    )
    (symbol "MX_SW_SOCKET_RGB_REV_1_1"
      (rectangle (start -6.35 0) (end 6.35 -8.89)
        (stroke (width 0) (type default))
        (fill (type background))
      )
      (rectangle (start -3.81 7.62) (end 3.81 1.27)
        (stroke (width 0) (type default))
        (fill (type background))
      )
      (circle (center -0.6173 5.0896) (radius 0.1705)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -1.27 5.08)
          (xy -1.27 7.62)
        )
        (stroke (width 0) (type dot))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.5184 5.2126)
          (xy 0.4381 5.7713)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 7.62)
          (xy 1.27 5.08)
        )
        (stroke (width 0) (type dot))
        (fill (type none))
      )
      (circle (center 0.6471 5.08) (radius 0.1705)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (text "NEOPIXEL" (at 0 -1.27 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "SWITCH" (at 0 2.54 0)
        (effects (font (size 1.27 1.27)))
      )
      (pin bidirectional line (at -1.27 10.16 270) (length 2.54)
        (name "L" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 1.27 10.16 270) (length 2.54)
        (name "R" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -11.43 90) (length 2.54)
        (name "G" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 -11.43 90) (length 2.54)
        (name "5V" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -8.89 -3.81 0) (length 2.54)
        (name "DIN" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 8.89 -3.81 180) (length 2.54)
        (name "DOUT" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
